                     UMC Motherboard Fix
               -------------------------------
                              
If you are using a UMC 486 motherboard  with the  Graphics Blaster  3D
series  cards, you might experience garbage appearing on  the  screen.
This  is  a  known  incompatibility problem  between  that  particular
revision of the motherboard with our PCI VGA card. This problem can be
solved by running the UMCFIX.EXE.

If  running UMCFIX.EXE solves the problem, you may like to put the fix
into  your system. To do that, you have to copy the UMCFIX.EXE to your
system   and   modify   your   Autoexec.bat   by   adding   the   line
C:\GB3D\umcfix.exe (assuming that C:\GB3D is the path where you copied
the file).

   -------------------- End of Text ----------------------
